Installation Instructions
	1.	Copy Keen.fw to the SD card and place it in the folder /odroid/firmware/
	2.	Create a folder on the SD card: /data/keen/
	3.	Download the CloneKeen source code and extract it to a temporary folder:

http://clonekeen.sourceforge.net/files/clonekeen-src-84.tar.gz

	4.	Open the extracted CloneKeen source folder and navigate to: /keen/bin/
	5.	Copy everything from this folder to /data/keen/ on the SD Card.
	6.	Copy all the files from the Full version or Shareware Commander Keen Episodes 1, 2 & 3 to the SD card folder: /data/keen/data/
	7.	Put the SD card in the Odroid-Go, then start while holding B.
	8.	Flash the Keen firmware.

Example SD card files:
	•	/odroid/firmware/Keen.fw
	•	/data/keen/keen.conf
	•	/data/keen/palette.ini
	•	/data/keen/strings.dat
	•	/data/keen/...
	•	/data/keen/data/CTLPANEL.CK1
	•	/data/keen/data/CTLPANEL.CK2
	•	/data/keen/data/CTLPANEL.CK3
	•	/data/keen/data/...
	•	/data/keen/gfx/100.tga
	•	/data/keen/gfx/200.tga
	•	/data/keen/gfx/500.tga
	•	/data/keen/gfx/...

Troubleshooting
If you have problems starting up, have a look at the log file: /data/keen/ck.log
It may have more information on what your problem is.