frodo-go
Commodore 64 emulation for ODROID-GO
To use, you will need to do the following steps:
	1.	Purchase and receive the ODROID-GO QWERTY Keyboard which is required for this emulator.
	2.	Create the below directory on your SD card. /roms/c64/
	3.	Place the following 4 BIOS files in the /roms/c64/ directory, named exactly as shown.
1541.ROM
Basic.ROM
Char.ROM
Kernal.ROM

	4.	Place your .D64 files in the /roms/c64/ directory. Only D64 format is supported at this time.
	5.	Displays error screen if keyboard not found, requires QWERTY keyboard.

Errata:

H = "HOME / CLR"
RE = "RESTORE"
RS = "Right Shift"